# Get

## Function

This API is used to get AI > Cross Counting Scenario > Config configuration parameters.

## Request Message

### Parameter Description

Table 1

Parameter | Range | Type | Description
--- | --- | --- | ---
channel | “CH1”…”CH1x” “IP_CH1”…” IP_CH1x” “WIFI_CH1”…” WIFI_CH1x” The number of channels depends on the capabilities of the device. | string array | Each array bit represents a channel with a string. DVR/NVR need; IPC only use CH1

Sample:

    POST /API/AI/Scenario/CC/Config/Get HTTP/1.1

    {
        "result": "success",
        "data": {
            ["CH1"]
        }
    }

## Response Message

### Parameter Description

Table 2

Parameter | Range | Type | Description
--- | --- | --- | ---
adSwitch |  | bool | Advertising mode control switch
ad_displayMode |  | bool | Keep aspect ratio switch
ad_seqTime |  | int | Ad image polling time
channel_info |  | JSON object | Channel Information JSON show as follow Table 3
group_info |  | JSON object | Group Information JSON show as follow Table 4

Table 3

Parameter | Range | Type | Description
--- | --- | --- | ---
channel_switch |  | bool | Control whether to open the CC scene application function
channel_group |  | int | The group number to which the channel belongs, and -1 if not in the group
channel_capacity |  | int | Capacity
chn_set_enable |  | bool | Whether the channel can be set or not is associated with the second-generation CC function
chn_buzzer | "0","10","20","40","60" | string | Buzzer sounding time
chn_alarm_out | “Local->1”… ”Local->x” “IP_CH1->1”… “IP_CH1->2”… ” IP_CHx->1” ” IP_CHx->2” The number of channels depends on the capabilities of the device. | array | Alarm output channel Each array bit represents aalarm output channel with a string. Camera: Local->1: open, empty value: close
chn_latch_time | "10","20","40","60" | string | Alarm output delay time

Table 4

Parameter | Range | Type | Description
--- | --- | --- | ---
group_switch |  | bool | Control whether to open the CC scene application function
group_capacity |  | int | Capacity
start_time | 8 | string | Starting time
end_time | 8 | string | End Time
alarm_type | "Unuse","Person","Vehicle" | string | alarm type: 1：Person，2：Vehicle
grp_buzzer | "0","10","20","40","60" | string | Buzzer sounding time
grp_alarm_out | “Local->1”… ”Local->x” “IP_CH1->1”… “IP_CH1->2”… ” IP_CHx->1” ” IP_CHx->2” The number of channels depends on the capabilities of the device. | array | Alarm output channel Each array bit represents aalarm output channel with a string. Camera: Local->1: open, empty value: close
grp_latch_time | "10","20","40","60" | string | Alarm output delay time

Sample:

    HTTP/1.1 200 OK
    Content-Type: application/json

    {
        "version": "success",
        "data": {
            "adSwitch": false,
            "ad_displayMode": false,
            "ad_seqTime": 1,
            "channel_info": {
                "CH1": {
                    "channel_switch": false,
                    "channel_group": -1,
                    "channel_capacity": 11,
                    "chn_set_enable": false,
                    "chn_buzzer": "0",
                    "chn_alarm_out": [],
                    "chn_latch_time": "20"
                },
                "CH8": {
                    "channel_switch": false,
                    "channel_group": 4,
                    "channel_capacity": 33,
                    "chn_set_enable": false,
                    "chn_buzzer": "0",
                    "chn_alarm_out": [],
                    "chn_latch_time": "10"
                }
            },
            "group_info": {
                "Group1": {
                    "group_switch": false,
                    "group_capacity": 30,
                    "start_time": "00:00:00",
                    "end_time": "23:59:59",
                    "alarm_type": "Person",
                    "grp_buzzer": "0",
                    "grp_alarm_out": [],
                    "grp_latch_time": "10"
                },
                "Group8": {
                    "group_switch": false,
                    "group_capacity": 10,
                    "start_time": "00:00:00",
                    "end_time": "23:59:29",
                    "alarm_type": "Person",
                    "grp_buzzer": "0",
                    "grp_alarm_out": [],
                    "grp_latch_time": "10"
                }
            }
        }
    }

## Error Code

See Response Messages Body and Common error_code for more information.