# IP Speaker Onvif

## Function

This API is used to get or set IP Speaker page parameters.

## URI

    POST /API/AlarmConfig/IpSpeakerOnvif/{Action}

Table 1 describes the parameters.

## describes the parameters.

Table 1

Parameter | Required | Description
--- | --- | ---
Action | yes | equest actions, including Range，Get，Set。
speaker | no | Range/Get/Set Request action can be brought"speaker":"SP1" Indicates the device name that operates only the SP1 device