# Get

## Function

This API is used to get PTZ control information.

## Request Message

### Parameter Description

##### Table 1

Parameter | Range | Type | Description
--- | --- | --- | ---
channel | "CH1"…"CHx", "IP_CH1"…" IP_CHx", "WIFI_CH1"…",WIFI_CHx", The number of channels depends on the capabilities of the device. | string | Channel name.

Sample:

    POST /API/PreviewChannel/PTZ/Get HTTP/1.1

    {
        "version": "1.0",
        "data":{
            "channel": "CH1",
            "disable_ManualHumanTrace": false,
            "current_cruise_mode": "Mode_Default_Cruise",
            "zoom_step": 5,
            "focus_step": 5
        }
    }

## Response Message

### Parameter Description

##### Table 2

Parameter | Range | Type | Description
--- | --- | --- | ---
channel |  | string |
ptz_version | "1.0","2.0","3.0" | string | Ptz version.
cmd | "Ptz_Cmd_Up", "Ptz_Cmd_Down", … … "Ptz_Privacy_Mode", "Ptz_Trace_Mode" | string | See Table 3 for more information of cmd.
state | "Stop","Start" | string | For button press and release.
support_autoCalibration |  | bool | Auto Calibration.
zoom_step | 1,5,20 | int | Zoom adjust the number of steps.
focus_step | 1,5,20 | int | Focus adjust the number of steps.
zoom_slider | Depending on the lens | int | Zoom slider.
focus_slider | Depending on the lens | int | Focus slider.
isctl |  | bool | Whether gray screen; true: no gray screen; false: gray screen.
speed | 0-10 0-100(For DVR/NVR) | int | (only control)
preset_point | 0-255 | int array | The maximum length of the array is 255, each bit represents a preset point, the value of each bit (0-255) represents the polling time of the corresponding preset point, 0 means no preset point is set for this bit.
line_scan_state |  | bool | Line scan cruise state.
trace_preset_point |  | array | Preset point set by TOUR.
preset_point_no | 1-255 | int | (only control)
ctl_stop |  | bool | true:stop ctl operation(only control)
preset_point_time | 1-255 | int | Single preset point polling time.(only control)
preset_point_name | len:1-31 | string | Preset point name, ranging from 1 to 31 character.
zoom_minus_add | "Ptz_Cmd_ZoomMinus" "Ptz_Cmd_ZoomAdd" | object | Range used it to display the zoom button
focus_minus_add | "Ptz_Cmd_FocusMinus", "Ptz_Cmd_FocusAdd" | object | Range used it to display the focus button Range
iris_minus_add | "Ptz_Cmd_IrisMinus", "Ptz_Cmd_IrisAdd" | object | Range used it to display aperture buttons.
btn_autofocus | "Ptz_Btn_AutoFocus" | object | Used to display the autofocus button.
btn_default | "Ptz_Btn_Default" | object | Used to display the restore button.
btn_refresh | "Ptz_Btn_Refresh" | object | Used to display the refresh button
preset_point_cruise_btn | "Ptz_Cmd_Cruise" | object | Used to display the cruise buttons.
is_req_progress |  | bool | Whether to issue the progress polling command.
ptz_direction_control | "Ptz_Cmd_Up" "Ptz_Cmd_Down", "Ptz_Cmd_Left", "Ptz_Cmd_Right", "Ptz_Cmd_UpLeft", "Ptz_Cmd_UpRight", "Ptz_Cmd_DownLeft", "Ptz_Cmd_DownRight", "Ptz_Cmd_CircleCenter" | object | Range used it to display direction control.
advanced_mode | "Mode_Preset_Point", "Mode_Watch_Mode", "Mode_Line_Scan", "Mode_Trace", "Mode_Pattern_Scan" | object | Range used it to display each mode in the advanced mode.
trace_number | 0-3 | int | Tour 1-4 tracks.
pattern_scan_number | 0-3 | int | Pattern scan 1-4 tracks.
pattern_scan_number_isset | 0-3 | bool array | Whether pattern scan 1-4 has been marked.
line_scan_speed | "Low", "Middle", "High" | string | line scan speed
line_scan_area |  | bool | Whether linear scan is set.
trace_interval | "5s""6s""7s"….."59s""60s" | string | Tour time interval.
utc_protocol |  | string | Utc Protocol.
utc_cmd | "Coax_Cmd_Menu", "Coax_Cmd_Up", | "Coax_Cmd_Left", "Coax_Cmd_Right", "Coax_Cmd_Down" | string
current_cruise_mode | "Mode_Default_Cruise", "Mode_Preset_Point", "Mode_Watch_Mode", "Mode_Line_Scan", "Mode_Trace", "Mode_Pattern_Scan", "Mode_Restore_Btn", "Mode_Auto_Scan" | string | Current pattern scan mode
belt_times_use | 0-100 | int | Belt life, more than 90, prompt life is not enough, 100 can not cruise.
quick_use | "Ptz_QuickUse_3DPosition", "Ptz_QuickUse_AutoFocus", "Ptz_QuickUse_PtzReset", "Ptz_QuickUse_WatchMode", "Ptz_QuickUse_ManualHumanTrace", "Ptz_QuickUse_LensReset" | string | Range used it to display shortcut function buttons.
preset_point_obj | 0-256 | object array | Object of the number of preset point arrays,see Table 4 for more information of member in array.
watch_mode_mode | "Mode_Default_Cruise", "Mode_Watch_Point", "Mode_Line_Scan", "Mode_Trace", "Mode_Pattern_Scan" | string | Mode of watch mode.
watch_mode_num | 0 - 255 | int | Num of public modes in watch mode.(except linear scan)
watch_mode_num | "low", "middle", "high" | string | Linear scan speed in watch mode.
disable_ManualHumanTrace |  | bool | Disable tracking of humans and vehicles.
point_times_use | 0 - 100 | int | The service life of the dome camera.

##### Table 3

Parameter | Range | Type | Description
--- | --- | --- | ---
cmd | "Ptz_Cmd_Up", "Ptz_Cmd_Down", "Ptz_Cmd_Left", "Ptz_Cmd_Right", "Ptz_Cmd_UpLeft", "Ptz_Cmd_UpRight", "Ptz_Cmd_DownLeft", "Ptz_Cmd_DownRight", "Ptz_Cmd_ZoomAdd", "Ptz_Cmd_ZoomMinus", "Ptz_Cmd_FocusAdd", "Ptz_Cmd_FocusMinus", "Ptz_Cmd_IrisAdd", "Ptz_Cmd_IrisMinus", "Ptz_Cmd_CircleCenter", "Ptz_Cmd_Cruise", "Ptz_Change_CruiseTime", "Ptz_Cmd_AddPreset", "Ptz_Cmd_ClearPreset", "Ptz_Cmd_CallPreset", "Ptz_Cmd_AuxiliartOpen", "Ptz_Cmd_AuxiliartClose", "Ptz_Cmd_LockFocus", "Ptz_LineScan_StartPoint", "Ptz_LineScan_EndPoint", "Ptz_Cmd_LineScanSetSpeed", "Ptz_LineScan_CruiseStart", "Ptz_LineScan_CruiseStop", "Ptz_Btn_Default", "Ptz_Zoom_Position", "Ptz_Focus_Position", "Ptz_Zoom_Move", "Ptz_Focus_Move", "Ptz_Btn_AutoFocus", "Ptz_AreaFocus", "Ptz_Btn_Refresh", "Ptz_CalibRationSetting", "Ptz_Tour_Start", "Ptz_Tour_Stop", "Ptz_Pattern_CruiseStart", "Ptz_Pattern_CruiseStop", "Ptz_Pattern_RecordStart", "Ptz_Pattern_RecordStop", "Ptz_Net_Osd", "Ptz_3Dposition", "Ptz_Light", "Ptz_Rain", "Ptz_CalcpadNumSetting", "Ptz_Cmd_NewSceneCalib", "Ptz_Cmd_DefCruise_Start", "Ptz_Cmd_DefCruise_Stop", "Ptz_WatchPoint_Add", "Ptz_Privacy_Mode", "Ptz_Trace_Mode" "Ptz_Cmd_AutoCalibration" | string | (only control)

##### Table 4

Parameter | Range | Type | Description
--- | --- | --- | ---
no | 1-256 | int | The number of preset points can be set up to 255.
name | len:1-31 | string | Array preset point name: range 1 to 31 character.
add |  | bool | Whether the preset point has been set.

Sample:

    HTTP/1.1 200 OK
    Content-Type: application/json

    {
        "result":"success",
        "data":{
            "channel":"CH1",
            "preset_point":[0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0],
            "belt_times_use":0,
            "preset_point_obj":
            [
                {
                    "no":1,
                    "name":"point 1",
                    "add":false
                },
                {
                    "no":2,
                    "name":"point 2",
                    "add":false
                },
                {
                    "no":3,
                    "name":"point 3",
                    "add":false
                },
                ...
                {
                    "no":254,
                    "name":"point 254",
                    "add":false
                },
                {
                    "no":255,
                    "name":"point 255",
                    "add":false
                }
            ],
            "watch_mode_time":20,
            "watch_mode_mode":"Mode_Default_Cruise",
            "watch_mode_num":0,
            "line_scan_area":false,
            "line_scan_speed":"low",
            "trace_interval":20,
            "trace_number":0,
            "trace_preset_point":[[],[],[],[]],
            "pattern_scan_number_isset":[true,false,false,false],
            "pattern_scan_number":0,
            "current_cruise_mode":"No_Cruise"
        }
    }

## Error Code

See Response Messages Body and Common error_code for more information.