# Set

## Function

This API is used to set Thermal > Measurement parameter.

## Request Message

### Parameter Description

See Thermal > Measurement > Request Message >Parameter Description > Table 2 Obtain the parameter description.

Sample:

    POST /API/Thermal/Setup/Measurement/Set HTTP/1.1

    {
        "version": "1.0",
        "data": {
            "channel_info": {"CH2": {
                "status": "Online",
                "switch": true,
                "colorbar_switch": false,
                "display_temp_on_optical": false,
                "display_temp_on_stream": true,
                "display_max_temp": true,
                "display_min_temp": false,
                "display_average_temp": false,
                "display_pos": "Near Target",
                "spot_measurement": false,
                "temp_unit": "Degree Celsius",
                "emissivity": 0.96,
                "distance_unit": "Meter",
                "target_distance": 1,
                "reflective_temp": 20,
                "chn_index": "CH2",
                "page": "chn_measurement"
            }},
            "page_type": "ChannelConfig"
        }
    }

## Response Message

none

Sample:

    HTTP/1.1 200 OK
    Content-Type: application/json

    {
        "result": "success",
        "data": {}
    }

## Error Code

See Response message body and general error_code for more information.