# Get

## Function

This API is used to get Channel > PTZ page parameters.

## Request Message

None.

Sample:

    POST /API/ChannelConfig/PTZ/Get HTTP/1.1

    {
    	"version": "1.0",
    	"data": {}
    }

## Response Message

See Channel> PTZ > Parameter Description > Table 1 for parameter description.

Sample:

    HTTP/1.1 200 OK
    Content-Type: application/json

    {
    	"result": "success",
    	"data": {
    		"channel_info": {
    			"CH1": {
    				"signal_type": "Analog",
    				"protocol": "COAX1",
    				"baudrate": "9600",
    				"databit": "8",
    				"stopbit": "1",
    				"parity": "None",
    				"address": 1,
    				"copy_ch": "analog"
    			},
    			"CH2": {
    				"signal_type": "Analog",
    				"protocol": "COAX1",
    				"baudrate": "9600",
    				"databit": "8",
    				"stopbit": "1",
    				"parity": "None",
    				"address": 2,
    				"copy_ch": "analog"
    			},
    			"CH3": {
    				"signal_type": "Analog",
    				"protocol": "COAX1",
    				"baudrate": "9600",
    				"databit": "8",
    				"stopbit": "1",
    				"parity": "None",
    				"address": 3,
    				"copy_ch": "analog"
    			},
    			"CH4": {
    				"signal_type": "Analog",
    				"protocol": "COAX1",
    				"baudrate": "9600",
    				"databit": "8",
    				"stopbit": "1",
    				"parity": "None",
    				"address": 4,
    				"copy_ch": "analog"
    			},
    			"CH5": {
    				"signal_type": "Analog",
    				"protocol": "COAX1",
    				"baudrate": "9600",
    				"databit": "8",
    				"stopbit": "1",
    				"parity": "None",
    				"address": 5,
    				"copy_ch": "analog"
    			},
    			"CH6": {
    				"signal_type": "Analog",
    				"protocol": "COAX1",
    				"baudrate": "9600",
    				"databit": "8",
    				"stopbit": "1",
    				"parity": "None",
    				"address": 6,
    				"copy_ch": "analog"
    			},
    			"CH7": {
    				"signal_type": "Analog",
    				"protocol": "COAX1",
    				"baudrate": "9600",
    				"databit": "8",
    				"stopbit": "1",
    				"parity": "None",
    				"address": 7,
    				"copy_ch": "analog"
    			},
    			"CH8": {
    				"signal_type": "Analog",
    				"protocol": "COAX1",
    				"baudrate": "9600",
    				"databit": "8",
    				"stopbit": "1",
    				"parity": "None",
    				"address": 8,
    				"copy_ch": "analog"
    			},
    			"IP_CH1": {
    				"reason": "Not configured"
    			},
    			"IP_CH2": {
    				"reason": "Not support"
    			},
    			"IP_CH3": {
    				"reason": "Not configured"
    			},
    			"IP_CH4": {
    				"status": "Offline"
    			},
    			"IP_CH5": {
    				"reason": "Not support"
    			},
    			"IP_CH6": {
    				"reason": "Not configured"
    			},
    			"IP_CH7": {
    				"reason": "Not configured"
    			},
    			"IP_CH8": {
    				"reason": "Not configured"
    			},
    			"IP_CH9": {
    				"reason": "Not configured"
    			},
    			"IP_CH10": {
    				"reason": "Not configured"
    			},
    			"IP_CH11": {
    				"reason": "Not configured"
    			},
    			"IP_CH12": {
    				"reason": "Not configured"
    			}
    		}
    	}
    }

## Error Code

See Response Messages Body and Common error_code for more information.