# Get

## Function

This API is used to get parameter for System > System Information page.

## Request Message

None.

Sample:

    POST /API/SystemInfo/Base/Get HTTP/1.1

    {
        "version": "1.0",
        "data": {}
    }

## Response Message

### Parameter Description

#### Table 1

Parameter | Range | Type | Description
--- | --- | --- | ---
device_id |  | string | DeviceID
device_name |  | string | DeviceName
device_type |  | string | DeviceType
hardware_version |  | string | HardwareVersion
software_version |  | string | SoftwareVersion
build_time |  | string | release time
ie_client_version |  | string | IE Client Version
mcu_software_version |  | string | MCU software version
video_format | “PAL”, “NTSC” | string | Video Format
hdd_volume |  | string | HDD Volume
ip_address |  | string | IP Address
ipv6_address |  | string | IPv6 Address
web |  | string | Web Internal port ,Web external port
client |  | string | Client Internal port , Clientexternal port
mac_address |  | string | MAC Address
wireless_mac |  | string | Wireless MAC
p2p_id |  | string | P2P ID
p2p_switch |  | boolean |
network_state | “Connected”, “Unconnected” | string | Network connection status
serialNum |  | string | Serial Number(B18)
language |  | string | The current language of the device
flash_write_cnt |  | int | Total flash write times (cloud dedicated)
>Tips： |  |  |
> |  |  |
>Later products will integrate the web port and the client port, and the client port will not be opened and the item will be removed from the page. For example, do not consider this port when the customer performs development interconnection. |  |  |

Sample:

    HTTP/1.1 200 OK
    Content-Type: application/json

    {
    	"result": "success",
    	"data": {
    		"device_id": "000000",
    		"device_name": "admin",
    		"device_type": "N7516",
    		"hardware_version": "DM-448",
    		"software_version": "V8.2.3-20221014",
    		"ie_client_version": "V1.3.1.45",
    		"video_format": "NTSC",
    		"hdd_volume": "465G",
    		"ip_address": "172.16.10.49",
    		"ipv6_address": "fe80::8a26:1dff:feaa:8ee0 / 64",
    		"web": "80,80",
    		"client": "9000,9000",
    		"mac_address": "88-26-1D-AA-8E-E0",
    		"network_state": "Connected",
    		"iot_id": "",
    		"language": "English"
    	}
    }

## Error Code

See Response Messages Body and Common error_code for more information.