# Get

## Function

This API is used to get Alarm > Intelligent Analysis configuration parameters.

## Request Message

##### Table 1

Parameter | Range | Type | Description
--- | --- | --- | ---
channel | "CH1"…"CHx", "IP_CH1"…"IP_CHx", "WIFI_CH1"…"WIFI_CHx" The channels supported by the device. | string array | IPC doesn't need to bring this key.

Sample:

    POST /API/Intelligent/IntelligentAnalysis/Get HTTP/1.1

    {
        "version": "1.0",
        "data": {
        }
    }

## Response Message

See Alarm > IntelligentAnalysis > Range > Parameter Description > Table 1 for parameter description.

Sample:

    HTTP/1.1 200 OK
    Content-Type: application/json

    {
        "result": "success",
        "data": {
            "channel_info": {
                "CH16": {
                    "report_type": "Daily report",
                    "cross_type": "Number of in",
                    "detection_type": "Motion",
                    "ai_cross_count": true,
                    "search_date": "2023-08-25"
                }
            }
        }
    }

## Error Code

See Response Messages Body and Common error_code for more information.