# Get

## Function

This API is used to get parameter for System > Record Information page.

## Request Message

None.

Sample:

    POST /API/SystemInfo/Record/Get HTTP/1.1

    {
        "version": "1.0",
        "data": {}
    }

## Response Message

### Parameter Description

Table 1

Parameter | Range | Type | Description
--- | --- | --- | ---
channel_info |  | object | channel_info object,see Table 2 for more information

Table 2

Channel info object

Parameter | Range | Type | Description
--- | --- | --- | ---
channel | CH1 IP_CH1 WIFI_CH1 | object | channel Table 3 for more information

Table 3

Channel object

Parameter | Range | Type | Description
--- | --- | --- | ---
channel |  | string | Channel Number
record_state | On Off | string | Record State
record_switch |  | bool | Record Switch
stream_type | Mainstream Substream DualStream | string | Video stream type
resolution |  | string | Resolution:Format: “Main Stream Resolution / Sub Stream Resolution”
fps |  | string | IP Camera's mainstream frame rate.(/Fps)Format:”Main Stream FPS / Sub Stream FPS”
bitrate |  | string | IP Camera's mainstream bitrate rate.(/Kbps)Format:”Main Stream Bitrate / Sub Stream Bitrate”

Sample:

    HTTP/1.1 200 OK
    Content-Type: application/json

    {
        "result": "success",
        "data": {
            "channel_info": {
                "CH5": {
                    "record_state": "Off",
                    "record_switch": "Enable"
                },
                "CH6": {
                    "record_state": "Off",
                    "record_switch": "Enable"
                },
                "CH7": {
                    "record_state": "Off",
                    "record_switch": "Enable"
                },
                "CH8": {
                    "record_state": "On",
                    "record_switch": "Enable",
                    "stream_type": "DualStream",
                    "resolution": "1920x1080 | 1280x720",
                    "fps": "30Fps | 25Fps",
                    "bitrate": "2Mbps | 1024Kbps"
                },
                "CH11": {
                    "record_state": "Off",
                    "record_switch": "Enable"
                },
                "CH14": {
                    "record_state": "On",
                    "record_switch": "Enable",
                    "stream_type": "DualStream",
                    "resolution": "1920x1080 | 1280x720",
                    "fps": "25Fps | 25Fps",
                    "bitrate": "1024Kbps | 1024Kbps"
                },
                "CH15": {
                    "record_state": "Off",
                    "record_switch": "Enable"
                },
                "CH16": {
                    "record_state": "Off",
                    "record_switch": "Enable"
                }
            },
            "channel_max": 16
        }
    }

## Error Code

See Response Messages Body and Common error_code for more information.